CR4250

* Package Contents:
  + What’s in the Box
    - CR4250 or CR4250-PoE
    - C8 line cord
    - Information on how to get started with your product
    - Warranty information
    - Rubber feet (4) for desk mounting
* Connecting a Wired WAN
  + Connect your Ethernet WAN source to the WAN port of the CR4250 (Port 0 is default WAN. All ports are LAN/WAN switchable).
* Connecting the Power Source
  + Plug the provided power supply (100-240V, 50-60Hz; 1.7A max without PoE, 4.1A max with PoE) into an electrical outlet. Then connect the power supply to the router.
  + Ensure power is switched on (O = OFF, – = ON)
  + When you set the power switch to the ON ( – ) position; watch for the power LED to illuminate.