IBR950

* Package Contents
  + What's in the Box:
    - A high-performance, ruggedized IBR950 series mobile router with an embedded business-class LTE modem and integrated mounting plate
    - A three-meter locking power and GPIO cable (direct wire)
    - Two Extra SIM door screws
    - Safety, Warranty and Regulatory guide
* Connecting a Wired WAN
  + Connect your Ethernet WAN source to the WAN port (Port WAN is default WAN. All ports are LAN/WAN switchable).
* Insert an Activated SIM
  + Unscrew and remove the SIM cover from the router.
  + Insert the card into the SIM1 slot, metal contacts down and notch in. It will click into place. Depress again to remove.
  + Insert the secondary SIM card into the SIM2 slot if desired.
  + Replace the SIM door cover and secure with the screws.
* Attach the Antennas
  + Attach the two cellular modem antennas to the connectors (not included).
  + Do not over-tighten. The maximum recommended torque is 4 in-lbs.
  + Angle the antennas for optimal signal reception.
* Connect the Power Source
  + The 4-pin power/GPIO cable connects directly to the router and is intended for connecting to a DC power source. Refer to the following for pin configuration to ensure the cables are connected appropriately:

