CBA550

* Package Contents
  + What's in the Box:
    - One CBA550 Adapter with embedded 150M LTE modem
    - Two universal LTE antennas with SMA direct attach
    - One SIM door screw
    - Safety, Regulatory, and Warranty Guide
* Insert an Activated SIM
  + Slide the SIM door cover to the left to reveal the SIM slots.
  + Insert the SIM into the slot marked SIM-1 with the metal contacts up and notch in. It will click into place. Depress the SIM card to remove it.
  + Use SIM-2 for secondary/backup SIM.
  + Slide the SIM door cover to the right to cover the SIM slots.
  + Insert the screw into the closed SIM cover and tighten.
* Attach the Antennas
  + Attach the two cellular modem antennas to the connectors.
  + Hold the antenna straight and twist the base of the antenna to connect to the device.
  + Do not over-tighten. The maximum recommended torque is 4 in-lbs.
  + Angle the antennas for optimal signal reception.
* Connect the Power Source
  + The CBA550 is powered a PoE-enabled RJ45 cable.
  + Connect LAN port to PoE enabled networking equipment to Passthrough 3G/4G Internet to Ethernet and receive power.
    - NOTE: If the router does not support PoE or does not have a PoE capable port, use a PoE injector optional accessory between the CBA550 and the router for power.